{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["download"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"download","index":0,"n_rows":2,"n_cols":27,"rows_kept":2,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Part Type","Part Number","Manufacturer Part Number","Manufacturer","Description","Value","Tolerance","Power (Watts)","Composition","Features","Temperature Coefficient","Operating Temperature","Package / Case","Size / Dimension","Height (Max)","Schematic Part","PCB Footprint","ROHS","SMT","Unit","Datasheet","3D","Distributor","Unit Price (USD)","Part Status","Update","Note"]
["Thick Film",null,"RC0603JR-070RL","Yageo","RES|Thick Film|0603|0ΩJumper|1A","0Ω","Jumper","1/10W","Thick Film","Moisture Resistant","-","-55°C ~ 155°C","0603","1.60mm x 0.80mm","0.55mm","RESISTOR\\RESISTOR","R0603N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0603N.step","Digi-Key",0.00258,"Active","2019-8-27"]