{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["download"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"download","index":0,"n_rows":181,"n_cols":27,"rows_kept":181,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Part Type","Part Number","Manufacturer Part Number","Manufacturer","Description","Value","Tolerance","Power (Watts)","Composition","Features","Temperature Coefficient","Operating Temperature","Package / Case","Size / Dimension","Height (Max)","Schematic Part","PCB Footprint","ROHS","SMT","Unit","Datasheet","3D","Distributor","Unit Price (USD)","Part Status","Update","Note"]
["Thick Film",null,"RC0402JR-070RL","Yageo","RES|Thick Film|0402|0ΩJumper|1A","0Ω","Jumper","1/16W","Thick Film","Moisture Resistant","-","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00152,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-071K1L","Yageo","RES|Thick Film|0402|1.1KΩ±5%|1/16W|±100ppm/°C","1.1KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-071M1L","Yageo","RES|Thick Film|0402|1.1MΩ±5%|1/16W|±100ppm/°C","1.1MΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-071R1L","Yageo","RES|Thick Film|0402|1.1Ω±5%|1/16W|±200ppm/°C","1.1Ω","±5%","1/16W","Thick Film","Moisture Resistant","±200ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00201,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-071K2L","Yageo","RES|Thick Film|0402|1.2KΩ±5%|1/16W|±100ppm/°C","1.2KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-071M2L","Yageo","RES|Thick Film|0402|1.2MΩ±5%|1/16W|±100ppm/°C","1.2MΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-071R2L","Yageo","RES|Thick Film|0402|1.2Ω±5%|1/16W|±200ppm/°C","1.2Ω","±5%","1/16W","Thick Film","Moisture Resistant","±200ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00201,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-071K3L","Yageo","RES|Thick Film|0402|1.3KΩ±5%|1/16W|±100ppm/°C","1.3KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-071M3L","Yageo","RES|Thick Film|0402|1.3MΩ±5%|1/16W|±100ppm/°C","1.3MΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-071R3L","Yageo","RES|Thick Film|0402|1.3Ω±5%|1/16W|±200ppm/°C","1.3Ω","±5%","1/16W","Thick Film","Moisture Resistant","±200ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00201,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-071K5L","Yageo","RES|Thick Film|0402|1.5KΩ±5%|1/16W|±100ppm/°C","1.5KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-071M5L","Yageo","RES|Thick Film|0402|1.5MΩ±5%|1/16W|±100ppm/°C","1.5MΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-071R5L","Yageo","RES|Thick Film|0402|1.5Ω±5%|1/16W|±200ppm/°C","1.5Ω","±5%","1/16W","Thick Film","Moisture Resistant","±200ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00201,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-071K6L","Yageo","RES|Thick Film|0402|1.6KΩ±5%|1/16W|±100ppm/°C","1.6KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-071M6L","Yageo","RES|Thick Film|0402|1.6MΩ±5%|1/16W|±100ppm/°C","1.6MΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-071R6L","Yageo","RES|Thick Film|0402|1.6Ω±5%|1/16W|±200ppm/°C","1.6Ω","±5%","1/16W","Thick Film","Moisture Resistant","±200ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00201,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-071K8L","Yageo","RES|Thick Film|0402|1.8KΩ±5%|1/16W|±100ppm/°C","1.8KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-071M8L","Yageo","RES|Thick Film|0402|1.8MΩ±5%|1/16W|±100ppm/°C","1.8MΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-071R8L","Yageo","RES|Thick Film|0402|1.8Ω±5%|1/16W|±200ppm/°C","1.8Ω","±5%","1/16W","Thick Film","Moisture Resistant","±200ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00201,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07100KL","Yageo","RES|Thick Film|0402|100KΩ±5%|1/16W|±100ppm/°C","100KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07100RL","Yageo","RES|Thick Film|0402|100Ω±5%|1/16W|±100ppm/°C","100Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0710KL","Yageo","RES|Thick Film|0402|10KΩ±5%|1/16W|±100ppm/°C","10KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0710ML","Yageo","RES|Thick Film|0402|10MΩ±5%|1/16W|±100ppm/°C","10MΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0710RL","Yageo","RES|Thick Film|0402|10Ω±5%|1/16W|±200ppm/°C","10Ω","±5%","1/16W","Thick Film","Moisture Resistant","±200ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00201,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07110KL","Yageo","RES|Thick Film|0402|110KΩ±5%|1/16W|±100ppm/°C","110KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07110RL","Yageo","RES|Thick Film|0402|110Ω±5%|1/16W|±100ppm/°C","110Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0711KL","Yageo","RES|Thick Film|0402|11KΩ±5%|1/16W|±100ppm/°C","11KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0711ML","Yageo","RES|Thick Film|0402|11MΩ±5%|1/16W|±200ppm/°C","11MΩ","±5%","1/16W","Thick Film","Moisture Resistant","±200ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00698,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0711RL","Yageo","RES|Thick Film|0402|11Ω±5%|1/16W|±100ppm/°C","11Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07120KL","Yageo","RES|Thick Film|0402|120KΩ±5%|1/16W|±100ppm/°C","120KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07120RL","Yageo","RES|Thick Film|0402|120Ω±5%|1/16W|±100ppm/°C","120Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0712KL","Yageo","RES|Thick Film|0402|12KΩ±5%|1/16W|±100ppm/°C","12KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0712ML","Yageo","RES|Thick Film|0402|12MΩ±5%|1/16W|±200ppm/°C","12MΩ","±5%","1/16W","Thick Film","Moisture Resistant","±200ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00698,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0712RL","Yageo","RES|Thick Film|0402|12Ω±5%|1/16W|±100ppm/°C","12Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07130KL","Yageo","RES|Thick Film|0402|130KΩ±5%|1/16W|±100ppm/°C","130KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07130RL","Yageo","RES|Thick Film|0402|130Ω±5%|1/16W|±100ppm/°C","130Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0713KL","Yageo","RES|Thick Film|0402|13KΩ±5%|1/16W|±100ppm/°C","13KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0713ML","Yageo","RES|Thick Film|0402|13MΩ±5%|1/16W|±200ppm/°C","13MΩ","±5%","1/16W","Thick Film","Moisture Resistant","±200ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00698,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0713RL","Yageo","RES|Thick Film|0402|13Ω±5%|1/16W|±100ppm/°C","13Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07150KL","Yageo","RES|Thick Film|0402|150KΩ±5%|1/16W|±100ppm/°C","150KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07150RL","Yageo","RES|Thick Film|0402|150Ω±5%|1/16W|±100ppm/°C","150Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0715KL","Yageo","RES|Thick Film|0402|15KΩ±5%|1/16W|±100ppm/°C","15KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0715ML","Yageo","RES|Thick Film|0402|15MΩ±5%|1/16W|±200ppm/°C","15MΩ","±5%","1/16W","Thick Film","Moisture Resistant","±200ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00698,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0715RL","Yageo","RES|Thick Film|0402|15Ω±5%|1/16W|±100ppm/°C","15Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07160KL","Yageo","RES|Thick Film|0402|160KΩ±5%|1/16W|±100ppm/°C","160KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07160RL","Yageo","RES|Thick Film|0402|160Ω±5%|1/16W|±100ppm/°C","160Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0716KL","Yageo","RES|Thick Film|0402|16KΩ±5%|1/16W|±100ppm/°C","16KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0716ML","Yageo","RES|Thick Film|0402|16MΩ±5%|1/16W|±200ppm/°C","16MΩ","±5%","1/16W","Thick Film","Moisture Resistant","±200ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00698,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0716RL","Yageo","RES|Thick Film|0402|16Ω±5%|1/16W|±100ppm/°C","16Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07180KL","Yageo","RES|Thick Film|0402|180KΩ±5%|1/16W|±100ppm/°C","180KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07180RL","Yageo","RES|Thick Film|0402|180Ω±5%|1/16W|±100ppm/°C","180Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0718KL","Yageo","RES|Thick Film|0402|18KΩ±5%|1/16W|±100ppm/°C","18KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0718ML","Yageo","RES|Thick Film|0402|18MΩ±5%|1/16W|±200ppm/°C","18MΩ","±5%","1/16W","Thick Film","Moisture Resistant","±200ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00698,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0718RL","Yageo","RES|Thick Film|0402|18Ω±5%|1/16W|±100ppm/°C","18Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-071KL","Yageo","RES|Thick Film|0402|1KΩ±5%|1/16W|±100ppm/°C","1KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-071ML","Yageo","RES|Thick Film|0402|1MΩ±5%|1/16W|±100ppm/°C","1MΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-071RL","Yageo","RES|Thick Film|0402|1Ω±5%|1/16W|±200ppm/°C","1Ω","±5%","1/16W","Thick Film","Moisture Resistant","±200ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00201,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-072K1L","Yageo","RES|Thick Film|0402|2.1KΩ±5%|1/16W|±100ppm/°C","2.1KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-072K2L","Yageo","RES|Thick Film|0402|2.2KΩ±5%|1/16W|±100ppm/°C","2.2KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-072M2L","Yageo","RES|Thick Film|0402|2.2MΩ±5%|1/16W|±100ppm/°C","2.2MΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-072R2L","Yageo","RES|Thick Film|0402|2.2Ω±5%|1/16W|±200ppm/°C","2.2Ω","±5%","1/16W","Thick Film","Moisture Resistant","±200ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00201,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-072K4L","Yageo","RES|Thick Film|0402|2.4KΩ±5%|1/16W|±100ppm/°C","2.4KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-072M4L","Yageo","RES|Thick Film|0402|2.4MΩ±5%|1/16W|±100ppm/°C","2.4MΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-072R4L","Yageo","RES|Thick Film|0402|2.4Ω±5%|1/16W|±200ppm/°C","2.4Ω","±5%","1/16W","Thick Film","Moisture Resistant","±200ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00201,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-072K7L","Yageo","RES|Thick Film|0402|2.7KΩ±5%|1/16W|±100ppm/°C","2.7KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-072M7L","Yageo","RES|Thick Film|0402|2.7MΩ±5%|1/16W|±100ppm/°C","2.7MΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-072R7L","Yageo","RES|Thick Film|0402|2.7Ω±5%|1/16W|±200ppm/°C","2.7Ω","±5%","1/16W","Thick Film","Moisture Resistant","±200ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00201,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07200KL","Yageo","RES|Thick Film|0402|200KΩ±5%|1/16W|±100ppm/°C","200KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07200RL","Yageo","RES|Thick Film|0402|200Ω±5%|1/16W|±100ppm/°C","200Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0720KL","Yageo","RES|Thick Film|0402|20KΩ±5%|1/16W|±100ppm/°C","20KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0720ML","Yageo","RES|Thick Film|0402|20MΩ±5%|1/16W|±200ppm/°C","20MΩ","±5%","1/16W","Thick Film","Moisture Resistant","±200ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00698,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0720RL","Yageo","RES|Thick Film|0402|20Ω±5%|1/16W|±100ppm/°C","20Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07220KL","Yageo","RES|Thick Film|0402|220KΩ±5%|1/16W|±100ppm/°C","220KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07220RL","Yageo","RES|Thick Film|0402|220Ω±5%|1/16W|±100ppm/°C","220Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0722KL","Yageo","RES|Thick Film|0402|22KΩ±5%|1/16W|±100ppm/°C","22KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0722ML","Yageo","RES|Thick Film|0402|22MΩ±5%|1/16W|±200ppm/°C","22MΩ","±5%","1/16W","Thick Film","Moisture Resistant","±200ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00698,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0722RL","Yageo","RES|Thick Film|0402|22Ω±5%|1/16W|±100ppm/°C","22Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07240KL","Yageo","RES|Thick Film|0402|240KΩ±5%|1/16W|±100ppm/°C","240KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07240RL","Yageo","RES|Thick Film|0402|240Ω±5%|1/16W|±100ppm/°C","240Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0724KL","Yageo","RES|Thick Film|0402|24KΩ±5%|1/16W|±100ppm/°C","24KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0724RL","Yageo","RES|Thick Film|0402|24Ω±5%|1/16W|±100ppm/°C","24Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07270KL","Yageo","RES|Thick Film|0402|270KΩ±5%|1/16W|±100ppm/°C","270KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07270RL","Yageo","RES|Thick Film|0402|270Ω±5%|1/16W|±100ppm/°C","270Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0727KL","Yageo","RES|Thick Film|0402|27KΩ±5%|1/16W|±100ppm/°C","27KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0727RL","Yageo","RES|Thick Film|0402|27Ω±5%|1/16W|±100ppm/°C","27Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-072KL","Yageo","RES|Thick Film|0402|2KΩ±5%|1/16W|±100ppm/°C","2KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-072ML","Yageo","RES|Thick Film|0402|2MΩ±5%|1/16W|±100ppm/°C","2MΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-072RL","Yageo","RES|Thick Film|0402|2Ω±5%|1/16W|±200ppm/°C","2Ω","±5%","1/16W","Thick Film","Moisture Resistant","±200ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00201,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-073K3L","Yageo","RES|Thick Film|0402|3.3KΩ±5%|1/16W|±100ppm/°C","3.3KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-073M3L","Yageo","RES|Thick Film|0402|3.3MΩ±5%|1/16W|±100ppm/°C","3.3MΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-073R3L","Yageo","RES|Thick Film|0402|3.3Ω±5%|1/16W|±200ppm/°C","3.3Ω","±5%","1/16W","Thick Film","Moisture Resistant","±200ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00201,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-073K6L","Yageo","RES|Thick Film|0402|3.6KΩ±5%|1/16W|±100ppm/°C","3.6KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-073M6L","Yageo","RES|Thick Film|0402|3.6MΩ±5%|1/16W|±100ppm/°C","3.6MΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-073R6L","Yageo","RES|Thick Film|0402|3.6Ω±5%|1/16W|±200ppm/°C","3.6Ω","±5%","1/16W","Thick Film","Moisture Resistant","±200ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00201,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-073K9L","Yageo","RES|Thick Film|0402|3.9KΩ±5%|1/16W|±100ppm/°C","3.9KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-073M9L","Yageo","RES|Thick Film|0402|3.9MΩ±5%|1/16W|±100ppm/°C","3.9MΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-073R9L","Yageo","RES|Thick Film|0402|3.9Ω±5%|1/16W|±200ppm/°C","3.9Ω","±5%","1/16W","Thick Film","Moisture Resistant","±200ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00201,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07300KL","Yageo","RES|Thick Film|0402|300KΩ±5%|1/16W|±100ppm/°C","300KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07300RL","Yageo","RES|Thick Film|0402|300Ω±5%|1/16W|±100ppm/°C","300Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0730KL","Yageo","RES|Thick Film|0402|30KΩ±5%|1/16W|±100ppm/°C","30KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0730RL","Yageo","RES|Thick Film|0402|30Ω±5%|1/16W|±100ppm/°C","30Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07330KL","Yageo","RES|Thick Film|0402|330KΩ±5%|1/16W|±100ppm/°C","330KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07330RL","Yageo","RES|Thick Film|0402|330Ω±5%|1/16W|±100ppm/°C","330Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0733KL","Yageo","RES|Thick Film|0402|33KΩ±5%|1/16W|±100ppm/°C","33KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0733RL","Yageo","RES|Thick Film|0402|33Ω±5%|1/16W|±100ppm/°C","33Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07360KL","Yageo","RES|Thick Film|0402|360KΩ±5%|1/16W|±100ppm/°C","360KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07360RL","Yageo","RES|Thick Film|0402|360Ω±5%|1/16W|±100ppm/°C","360Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0736KL","Yageo","RES|Thick Film|0402|36KΩ±5%|1/16W|±100ppm/°C","36KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0736RL","Yageo","RES|Thick Film|0402|36Ω±5%|1/16W|±100ppm/°C","36Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07390KL","Yageo","RES|Thick Film|0402|390KΩ±5%|1/16W|±100ppm/°C","390KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07390RL","Yageo","RES|Thick Film|0402|390Ω±5%|1/16W|±100ppm/°C","390Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0739KL","Yageo","RES|Thick Film|0402|39KΩ±5%|1/16W|±100ppm/°C","39KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0739RL","Yageo","RES|Thick Film|0402|39Ω±5%|1/16W|±100ppm/°C","39Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-073KL","Yageo","RES|Thick Film|0402|3KΩ±5%|1/16W|±100ppm/°C","3KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-073ML","Yageo","RES|Thick Film|0402|3MΩ±5%|1/16W|±100ppm/°C","3MΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-073RL","Yageo","RES|Thick Film|0402|3Ω±5%|1/16W|±200ppm/°C","3Ω","±5%","1/16W","Thick Film","Moisture Resistant","±200ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00201,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-074K3L","Yageo","RES|Thick Film|0402|4.3KΩ±5%|1/16W|±100ppm/°C","4.3KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-074M3L","Yageo","RES|Thick Film|0402|4.3MΩ±5%|1/16W|±100ppm/°C","4.3MΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-074R3L","Yageo","RES|Thick Film|0402|4.3Ω±5%|1/16W|±200ppm/°C","4.3Ω","±5%","1/16W","Thick Film","Moisture Resistant","±200ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00201,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-074K7L","Yageo","RES|Thick Film|0402|4.7KΩ±5%|1/16W|±100ppm/°C","4.7KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-074M7L","Yageo","RES|Thick Film|0402|4.7MΩ±5%|1/16W|±100ppm/°C","4.7MΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-074R7L","Yageo","RES|Thick Film|0402|4.7Ω±5%|1/16W|±200ppm/°C","4.7Ω","±5%","1/16W","Thick Film","Moisture Resistant","±200ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00201,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07430KL","Yageo","RES|Thick Film|0402|430KΩ±5%|1/16W|±100ppm/°C","430KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07430RL","Yageo","RES|Thick Film|0402|430Ω±5%|1/16W|±100ppm/°C","430Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0743KL","Yageo","RES|Thick Film|0402|43KΩ±5%|1/16W|±100ppm/°C","43KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0743RL","Yageo","RES|Thick Film|0402|43Ω±5%|1/16W|±100ppm/°C","43Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07470KL","Yageo","RES|Thick Film|0402|470KΩ±5%|1/16W|±100ppm/°C","470KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07470RL","Yageo","RES|Thick Film|0402|470Ω±5%|1/16W|±100ppm/°C","470Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0747KL","Yageo","RES|Thick Film|0402|47KΩ±5%|1/16W|±100ppm/°C","47KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0747RL","Yageo","RES|Thick Film|0402|47Ω±5%|1/16W|±100ppm/°C","47Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-075K1L","Yageo","RES|Thick Film|0402|5.1KΩ±5%|1/16W|±100ppm/°C","5.1KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-075M1L","Yageo","RES|Thick Film|0402|5.1MΩ±5%|1/16W|±100ppm/°C","5.1MΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-075R1L","Yageo","RES|Thick Film|0402|5.1Ω±5%|1/16W|±200ppm/°C","5.1Ω","±5%","1/16W","Thick Film","Moisture Resistant","±200ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00201,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-075K6L","Yageo","RES|Thick Film|0402|5.6KΩ±5%|1/16W|±100ppm/°C","5.6KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-075M6L","Yageo","RES|Thick Film|0402|5.6MΩ±5%|1/16W|±100ppm/°C","5.6MΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-075R6L","Yageo","RES|Thick Film|0402|5.6Ω±5%|1/16W|±200ppm/°C","5.6Ω","±5%","1/16W","Thick Film","Moisture Resistant","±200ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00201,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0750RL","Yageo","RES|Thick Film|0402|50Ω±5%|1/16W|±100ppm/°C","50Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07510KL","Yageo","RES|Thick Film|0402|510KΩ±5%|1/16W|±100ppm/°C","510KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07510RL","Yageo","RES|Thick Film|0402|510Ω±5%|1/16W|±100ppm/°C","510Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0751KL","Yageo","RES|Thick Film|0402|51KΩ±5%|1/16W|±100ppm/°C","51KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0751RL","Yageo","RES|Thick Film|0402|51Ω±5%|1/16W|±100ppm/°C","51Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07560KL","Yageo","RES|Thick Film|0402|560KΩ±5%|1/16W|±100ppm/°C","560KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07560RL","Yageo","RES|Thick Film|0402|560Ω±5%|1/16W|±100ppm/°C","560Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0756KL","Yageo","RES|Thick Film|0402|56KΩ±5%|1/16W|±100ppm/°C","56KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0756RL","Yageo","RES|Thick Film|0402|56Ω±5%|1/16W|±100ppm/°C","56Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-076K2L","Yageo","RES|Thick Film|0402|6.2KΩ±5%|1/16W|±100ppm/°C","6.2KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-076M2L","Yageo","RES|Thick Film|0402|6.2MΩ±5%|1/16W|±100ppm/°C","6.2MΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-076R2L","Yageo","RES|Thick Film|0402|6.2Ω±5%|1/16W|±200ppm/°C","6.2Ω","±5%","1/16W","Thick Film","Moisture Resistant","±200ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00201,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-076K8L","Yageo","RES|Thick Film|0402|6.8KΩ±5%|1/16W|±100ppm/°C","6.8KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-076M8L","Yageo","RES|Thick Film|0402|6.8MΩ±5%|1/16W|±100ppm/°C","6.8MΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-076R8L","Yageo","RES|Thick Film|0402|6.8Ω±5%|1/16W|±200ppm/°C","6.8Ω","±5%","1/16W","Thick Film","Moisture Resistant","±200ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00201,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07620KL","Yageo","RES|Thick Film|0402|620KΩ±5%|1/16W|±100ppm/°C","620KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07620RL","Yageo","RES|Thick Film|0402|620Ω±5%|1/16W|±100ppm/°C","620Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0762KL","Yageo","RES|Thick Film|0402|62KΩ±5%|1/16W|±100ppm/°C","62KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0762RL","Yageo","RES|Thick Film|0402|62Ω±5%|1/16W|±100ppm/°C","62Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07680KL","Yageo","RES|Thick Film|0402|680KΩ±5%|1/16W|±100ppm/°C","680KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07680RL","Yageo","RES|Thick Film|0402|680Ω±5%|1/16W|±100ppm/°C","680Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0768KL","Yageo","RES|Thick Film|0402|68KΩ±5%|1/16W|±100ppm/°C","68KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0768RL","Yageo","RES|Thick Film|0402|68Ω±5%|1/16W|±100ppm/°C","68Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-077K5L","Yageo","RES|Thick Film|0402|7.5KΩ±5%|1/16W|±100ppm/°C","7.5KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-077M5L","Yageo","RES|Thick Film|0402|7.5MΩ±5%|1/16W|±100ppm/°C","7.5MΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-077R5L","Yageo","RES|Thick Film|0402|7.5Ω±5%|1/16W|±200ppm/°C","7.5Ω","±5%","1/16W","Thick Film","Moisture Resistant","±200ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00201,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07750KL","Yageo","RES|Thick Film|0402|750KΩ±5%|1/16W|±100ppm/°C","750KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07750RL","Yageo","RES|Thick Film|0402|750Ω±5%|1/16W|±100ppm/°C","750Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0775KL","Yageo","RES|Thick Film|0402|75KΩ±5%|1/16W|±100ppm/°C","75KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0775RL","Yageo","RES|Thick Film|0402|75Ω±5%|1/16W|±100ppm/°C","75Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-078K2L","Yageo","RES|Thick Film|0402|8.2KΩ±5%|1/16W|±100ppm/°C","8.2KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-078M2L","Yageo","RES|Thick Film|0402|8.2MΩ±5%|1/16W|±100ppm/°C","8.2MΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-078R2L","Yageo","RES|Thick Film|0402|8.2Ω±5%|1/16W|±200ppm/°C","8.2Ω","±5%","1/16W","Thick Film","Moisture Resistant","±200ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00201,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07820KL","Yageo","RES|Thick Film|0402|820KΩ±5%|1/16W|±100ppm/°C","820KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07820RL","Yageo","RES|Thick Film|0402|820Ω±5%|1/16W|±100ppm/°C","820Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0782KL","Yageo","RES|Thick Film|0402|82KΩ±5%|1/16W|±100ppm/°C","82KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0782RL","Yageo","RES|Thick Film|0402|82Ω±5%|1/16W|±100ppm/°C","82Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-079K1L","Yageo","RES|Thick Film|0402|9.1KΩ±5%|1/16W|±100ppm/°C","9.1KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-079M1L","Yageo","RES|Thick Film|0402|9.1MΩ±5%|1/16W|±100ppm/°C","9.1MΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-079R1L","Yageo","RES|Thick Film|0402|9.1Ω±5%|1/16W|±200ppm/°C","9.1Ω","±5%","1/16W","Thick Film","Moisture Resistant","±200ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00201,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07910KL","Yageo","RES|Thick Film|0402|910KΩ±5%|1/16W|±100ppm/°C","910KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-07910RL","Yageo","RES|Thick Film|0402|910Ω±5%|1/16W|±100ppm/°C","910Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0791KL","Yageo","RES|Thick Film|0402|91KΩ±5%|1/16W|±100ppm/°C","91KΩ","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]
["Thick Film",null,"RC0402JR-0791RL","Yageo","RES|Thick Film|0402|91Ω±5%|1/16W|±100ppm/°C","91Ω","±5%","1/16W","Thick Film","Moisture Resistant","±100ppm/°C","-55°C ~ 155°C","0402","1.00mm x 0.50mm","0.40mm","RESISTOR\\RESISTOR","R0402N","Yes","Yes","PCS","PYu-RC_Group_51_RoHS_L_10.pdf","R0402N.step","Digi-Key",0.00139,"Active","2019-8-8"]